{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":6,"rows_kept":3,"merged":[[0,0,0,5]]}
["大学江津校区光缆租用询价单\n（2023-JLJYAH-F4001）"]
["序号","租用需求","主要技术参数","售后服务需求","其他说明","报价"]
[1,"满足大学江津校区通信机房至某单位通信机房的通联（全程18公里）。","1.满足1000M以上传输，光衰0.2db每公里；\n2.纯裸光缆（12芯），中间不得有任何设备转接，可通过红光笔测试。\n","出现线路故障，30分钟内响应处理,2小时内完成故障处理。","合同有效期为1年。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}